Miscellaneous 
DEPARTMENT OF ENVIRONMENTAL PROTECTION
Notice of Completed Rule Review

RULE NOS.:
RULE TITLES:

62-18.060
Meter Operation

62-18.070
Highway Measurement Sites

Notice is hereby given that on August 26, 2026, the above rules completed the rule review process pursuant to Section 120.5435, F.S.

The following rule was filed with technical changes:

62-18.070 Highway Measurement Sites.
Sites for measuring sound from vehicles operated on highways shall meet the following requirements:

(1) Standard Sites. Standard measuring sites shall be open and free of sound-reflecting surfaces within a 100ꞌ foot radius of the microphone and a 100ꞌ foot radius of the microphone point as shown in Figure 1.
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(2) Restricted Sites. Restricted measuring sites which do not meet standard site requirements because of large sound-reflecting surfaces within the clear area (see Figure 2) may be used by applying correction factors determined from the following procedure.
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Figure 2
(a) Distance from sound-reflecting surfaces. The distances between the microphone line and its nearest sound-reflecting surface and between the centerline of the lane of travel and its nearest sound-reflecting surface shall be measured. These distances shall be located on the nomogram in Figure 3 on their respective axes, and the two marks shall be connected by a straight line. The point on the central axis that is intersected by the straight line indicates the dB correction factor that shall be applied to the sound level reading obtained from each vehicle passing through the site. (The dotted line in Figure 3 illustrates a - 2dB correction for sound-reflecting surfaces at 52ꞌ feet from the center of the lane of travel and 25ꞌ feet from the microphone line.)

1. through 2. No change.

3. Sound-reflecting surfaces not basically parallel to the lane of travel shall be 100 feet or more from the microphone and microphone point. This restriction does not apply to surfaces that are perpendicular to the lane of travel and behind the parallel surface for which corrections are made, such as a fence, or the side walls of a building.
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(b) through (d) No change.

(3) through (4) No change.

Rulemaking Authority 403.061 FS. Law Implemented 403.061, 403.415(9), 316.293(3) FS. History–New 11-27-74, Formerly 17-18.07, 17-18.070, Reviewed            .
