Notice of Rule Development

WATER MANAGEMENT DISTRICTS
St. Johns River Water Management District
RULE NO.:
RULE TITLE:

40C-8.031
Minimum Surface Water Levels and Flows and Groundwater Levels

PURPOSE AND EFFECT: The purpose and effect of the proposed rule amendment will be to establish minimum surface water levels for Johns Lake in Lake and Orange counties and to clarify the location of Lakes Brooklyn and Geneva in Bradford and Clay counties. These minimum water levels, if adopted by rule, will represent the limit at which further withdrawals would be significantly harmful to the water resources of the area or ecology of the area. The proposed minimum water levels for Johns Lake will not be in prevention or recovery. Thus, they will not have an adverse impact on small businesses or increase regulatory costs.

SUBJECT AREA TO BE ADDRESSED: The proposed rule would establish minimum surface water levels for Johns Lake pursuant to the mandate of Section 373.042, Florida Statutes, and clarify the location of Lakes Brooklyn and Geneva. The terms used herein are already defined in Chapter 40C-8, F.A.C. As with all minimum surface water levels established by the District, if adopted, the minimum surface water levels in this rule amendment would be used as a basis for imposing limitations on withdrawals of groundwater and surface water in the consumptive use permit regulatory process and for reviewing proposed surface water management systems in the environmental resource permit regulatory process.

RULEMAKING AUTHORITY: 373.042, 373.044, 373.113, F.S.

LAW IMPLEMENTED: 373.042, 373.0421, F.S.

IF REQUESTED IN WRITING AND NOT DEEMED UNNECESSARY BY THE AGENCY HEAD, A RULE DEVELOPMENT WORKSHOP WILL BE NOTICED IN THE NEXT AVAILABLE FLORIDA ADMINISTRATIVE REGISTER.

THE PERSON TO BE CONTACTED REGARDING THE PROPOSED RULE DEVELOPMENT AND A COPY OF THE PRELIMINARY DRAFT, IF AVAILABLE, IS: Tom Mayton, Deputy General Counsel, St. Johns River Water Management District, Office of General Counsel, 4049 Reid Street, Palatka, Florida 32177, (386)329-4108 tmayton@sjrwmd.com. TO REQUEST A RULE DEVELOPMENT WORKSHOP, CONTACT TOM MAYTON WITHIN 21 DAYS OF PUBLICATION OF THIS NOTICE.

THE PRELIMINARY TEXT OF THE PROPOSED RULE DEVELOPMENT IS:

40C-8.031 Minimum Surface Water Levels and Flows and Groundwater Levels.
(1) through (4) No change.
(5) The following minimum surface water levels are established as exceedance percentiles:
	System Name
	County
	Minimum Level
	Level
(ft NAVD)

	Apshawa South
	Lake
	P25
	83.6

	 
	P50
	82.3

	
	P75
	80.8

	Brooklyn
	Bradford and Clay
	P25
	111.5

	 
	P50
	106.2

	
	P75
	98.6

	Butler
	Volusia 
	P50
	20.1

	Geneva
	Bradford and Clay 
	P25
	101.7

	Clay
	P50
	98.3

	
	P75
	89.3

	Johns Lake
	Lake and Orange
	P25
	94.8

	 
	 
	P50
	93.7

	 
	 
	P75
	92.2

	Lochloosa
	Alachua
	P50
	56.5


The minimum P25, P50, and P75 levels for Apshawa Lake South are based on the MFLs condition lake level time series (1/27/1959 – 12/31/2018), effective {February 2025} which is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-17728 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529. 
MFL status of Apshawa Lake South will be assessed by comparing the minimum P25, P50, and P75 to the current P25, P50, and P75, respectively. The current P25, P50, and P75 for Apshawa Lake South are calculated by updating the current-pumping condition lake level time series (1/27/1959 – 12/31/2018) with post-2018 observed data at SJRWMD gage 2930258. The current-pumping condition lake level time series is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-17728 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
The minimum P25, P50, and P75 levels for Lake Brooklyn are based on the MFLs condition lake level time series (7/17/1957 – 12/31/2018), effective 9/28/2021, which is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-13524 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529. 
MFL status of Lake Brooklyn will be assessed by comparing the minimum P25, P50, and P75 to the current P25, P50, and P75, respectively. The current P25, P50, and P75 for Lake Brooklyn are calculated by updating the current-pumping condition lake level time series (7/17/1957 – 12/31/2018) with post-2018 observed data at SJRWMD gage 3360373. The current-pumping condition lake level time series is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-13524 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
The minimum P50 level for Lake Butler is a long-term median lake level based on the MFLs condition lake level time series (1949 – 2018), effective September 30, 2020, which is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-12168 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
MFL status of Lake Butler will be assessed by comparing the minimum P50 to the current P50. The current P50 for Lake Butler is calculated by updating the simulated historical lake level time series (1949 – 2018) with post-2018 observed data at SJRWMD gage 03390378. The simulated historical lake level time series is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-12168 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
The minimum P25, P50, and P75 levels for Lake Geneva are based on the MFLs condition lake level time series (7/1/1957 – 12/31/2018), effective 9/28/2021, which is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-13525 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
MFL status of Lake Geneva will be assessed by comparing the minimum P25, P50, and P75 to the current P25, P50, and P75, respectively. The current P25, P50, and P75 for Lake Geneva are calculated by updating the current-pumping condition lake level time series (7/1/1957 – 12/31/2018) with post-2018 observed data at SJRWMD gage 11590497. The current-pumping condition lake level time series is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-13525 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
The minimum P25, P50, and P75 levels for Johns Lake are based on the MFLs condition lake level time series (1/1/1948 – 12/31/2020), effective {effective date}, which is incorporated by reference and available at https://flrules.org/Gateway/reference.asp?No=Ref-20147 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529. 
MFL status of Johns Lake will be assessed by comparing the minimum P25, P50, and P75 to the current P25, P50, and P75, respectively. The current P25, P50, and P75 for Johns Lake are calculated by updating the current-pumping condition lake level time series (1/1/1948 – 12/31/2020) with post-2020 observed data at SJRWMD gage 03840562. The current-pumping condition lake level time series is incorporated by reference and available at https://flrules.org/Gateway/reference.asp?No=Ref-20147 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
The minimum P50 level for Lochloosa Lake is a long-term median lake level based on the MFLs condition lake level time series (1957 – 2015), effective 1-30-19, which is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-10225 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
MFL status of Lochloosa Lake will be assessed by comparing the minimum P50 to the current P50. The current P50 for Lochloosa Lake is calculated by updating the simulated historical lake level time series (1957 – 2015) with post-2015 observed data at SJRWMD gage 71481615. The simulated historical lake level time series is incorporated by reference and available at https://www.flrules.org/Gateway/reference.asp?No=Ref-10225 and upon request from the St. Johns River Water Management District, 4049 Reid Street, Palatka, FL 32177-2529.
(6) through (13) No change. 
Rulemaking Authority 373.042, 373.044, 373.113 FS. Law Implemented 373.042, 373.0421, 373.103, 373.415 FS. History–New 9-16-92, Amended 8-17-94, 6-8-95, 1-17-96, 8-20-96, 10-20-96, 11-4-98, 6-27-00, 2-13-01, 3-19-02, 5-12-03, 11-10-03, 1-12-04, 2-1-06, 12-3-06, 5-10-07, 5-24-07, 1-11-10, 8-22-13, 4-3-14, 11-25-14, 12-31-14, 1-31-16 (4)(aaa), 1-31-16 (4)(ssss), 2-1-17 (4)(w), 2-1-17 (6), (8), 6-27-17 (7), 6-29-17 (5), (8), (9), 1-30-19, 9-30-20, 9-28-21, 2-24-25, effective date.
