Miscellaneous 
DEPARTMENT OF ENVIRONMENTAL PROTECTION
Notice of Completed Rule Review

RULE NOS.:
RULE TITLES:

62-640.100
Scope, Intent, Purpose, and Applicability

62-640.200
Definitions

62-640.210
General Technical Guidance and Forms

62-640.300
General Requirements

62-640.400
Prohibitions

62-640.500
Nutrient Management Plan (NMP)

62-640.600
Pathogen Reduction and Vector Attraction Reduction

62-640.650
Monitoring, Record Keeping, Reporting, and Notification

62-640.700
Requirements for Land Application

62-640.800
Additional Requirements for Land Application at Reclamation Sites

62-640.850
Distribution and Marketing of - Class AA Biosolids

62-640.860
Other Solids

62-640.880
Additional Requirements Related to Biosolids Treatment Facilities

Notice is hereby given that on September 10, 2026, the above rules completed the rule review process pursuant to Section 120.5435, F.S.

The following rules were filed with technical changes:

62-640.650 Monitoring, Record Keeping, Reporting, and Notification.

(1) through (2) No change. 
(3) Monitoring Requirements.

(a) Biosolids Monitoring.

1. Biosolids sampling and analysis shall be conducted as follows:

a. Monitoring for the pathogen and vector attraction reduction requirements of rule 62-640.600, F.A.C., and the parameters in subparagraph 62-640.650(3)(a)3., F.A.C., shall be conducted by the treatment facility in accordance with 40 C.F.R. 503.8, codified as of July 1, 2018, which the Department hereby adopts and incorporates by reference available at http://www.flrules.org/Gateway/reference.asp?No=Ref-13259, and the POTW Sludge Sampling and Analysis Guidance Document, U.S. Environmental Protection Agency, August 1989, which the Department adopts and incorporates by reference available at http://flrules.org/Gateway/reference.asp?No=Ref-20015 http://www.flrules.org/Gateway/reference.asp?No=Ref-13258. These documents are also available from the Wastewater Management Program, M.S. 3545, 2600 Blair Stone Road, Tallahassee, Florida 32399-2400. In cases where disagreements exist between 40 C.F.R. 503.8 and the POTW Sludge Sampling and Analysis Guidance Document, the requirements in 40 C.F.R. 503.8 will apply.

b. through c. No change. 
2. through 7. No change.

(b) through (e) No change. 
(4) through (6) No change.

Rulemaking Authority 373.043, 403.051, 403.061, 403.062, 403.0855, 403.087, 403.088, 403.704, 403.707 FS. Law Implemented 373.4595, 403.021, 403.051, 403.061, 403.0855, 403.087, 403.088, 403.0881, 403.702, 403.704, 403.707, 403.708 FS. History–New 3-30-98, Amended 8-29-10, 6-21-21, Reviewed          . 
62-640.880 Additional Requirements Related to Biosolids Treatment Facilities.

The requirements of this section shall apply to any facility that treats biosolids from other facilities prior to use, land application, or disposal. These requirements also apply to septage management facilities that treat domestic septage and combinations of food establishment sludges, wastes removed from portable toilets, and wastes removed from holding tanks associated with boats, marina pumpout, or other onsite systems prior to use, land application, or disposal.

(1) No change. 
(2) Permitting.

(a) Fees. For the purpose of determining applicable permit fees, the biosolids treatment facility shall be classified as Type I, II, or III based on the design capacity established by the permittee as follows:

	Type
	Design Capacity (Dry Tons Per Year)
	Design Capacity (Dry Tons Per Day Year)

	I
	≥1,653
	≥4.5 

	II 
	320-1,653
	0.88-4.5 

	III
	≤320
	≤0.88 


(b) through (k) No change.

(3) through (6) No change. 
Rulemaking Authority 403.051, 403.061, 403.062, 403.0855, 403.087, 403.088, 403.704, 403.707 FS. Law Implemented 403.021, 403.051, 403.061, 403.0855, 403.087, 403.088, 403.0881, 403.702, 403.704, 403.707, 403.708 FS. History–New 3-30-98, Amended 8-29-10, 6-21-21, Reviewed         .
