Notice of Variances and Waivers

DEPARTMENT OF BUSINESS AND PROFESSIONAL REGULATION
Division of Hotels and Restaurants
RULE NO.:
RULE TITLE:

61C-5.001
Safety Standards

NOTICE OF DISPOSITION FOR VARIANCE OR WAIVER

NOTICE IS HEREBY GIVEN that on October 27, 2026, the Department of Business and Professional Regulation, Division of Hotels and Restaurants, Bureau of Elevator Safety, received a request to withdraw the Petition for Variance from NFI Industries filed May 18, 2026, and advertised on May 29, 2026, in Vol. 52 No. 104 of the Florida Administrative Register. The Petition requested a variance from Rule 2.7.1, ASME A18.1, 2020 edition, as adopted by Rule 61C-5.001, Florida Administrative Code, which requires that the rated load shall be not less than 250 kg (550 lb) nor more than 475 kg (1,050 lb). Platforms with a floor greater than 1.4 m2 (15 ft2) shall have a rated load of not less than 340 kg (750 lb). Platforms with a floor greater than 1.7 m2 (18 ft2) shall have a rated load of not less than 4 75 kg (1,050 lb). The lift shall be capable of sustaining and lowering a load as specified in Figure 9. 7. The rated speed shall not exceed 0.15 m/s (30 ft/min). The rated speed of lifts conforming to 2.1.6 shall not exceed 0.05 m/s (10 ft/min). Travel of lifts conforming to 2.1.1 and 2.1.2 shall not exceed 4 250 mm (168 in.). Travel of lifts conforming to 2.1.3 or shall not exceed 1 500 mm (60 in.). Travel of lifts conforming to 2.1.4 shall not exceed 600 mm (24 in.). Travel of lifts conforming to 2.1.6 shall not exceed 375 mm (15 in.), The Department of Business and Professional Regulation, Division of Hotels and Restaurants, Bureau of Elevator Safety, is taking no further action on the petition (VW2026-067).

A copy of the Order may be obtained by contacting: Division of Hotels and Restaurants, Bureau of Elevator Safety, 2601 Blair Stone Road, Tallahassee, Florida 32399-1013, dhr.elevators@myfloridalicense.com.

