Notice of Variances and Waivers

DEPARTMENT OF BUSINESS AND PROFESSIONAL REGULATION
Division of Hotels and Restaurants
RULE NO.:
RULE TITLE:

61C-5.001
Safety Standards

NOTICE OF PETITION FOR VARIANCE OR WAIVER

NOTICE IS HEREBY GIVEN that on October 15, 2026, the Department of Business and Professional Regulation, Division of Hotels and Restaurants, Bureau of Elevator Safety, received a petition for a routine variance from Lands End Village Condominium Association at 1642 Land’s End Village, Captiva, FL 33924. 

Petitioner seeks a routine variance from the requirements of ASME A18.1, 2020 Edition, Section 2.7.1, as adopted by 61C-5.001, Florida Administrative Code, which requires that the rated load shall be not less than 250 kg (550 lb) nor more than 475 kg (1,050 lb). Platforms with a floor greater than 1.4 m2 (15 ft2) shall have a rated load of not less than 340 kg (750 lb). Platforms with a floor greater than 1.7 m2 (18 ft2) shall have a rated load of not less than 4 75 kg (1,050 lb). The lift shall be capable of sustaining and lowering a load as specified in Figure 9. 7. The rated speed shall not exceed 0.15 m/s (30 ft/min). The rated speed of lifts conforming to 2.1.6 shall not exceed 0.05 m/s (10 ft/min). Travel of lifts conforming to 2.1.1 and 2.1.2 shall not exceed 4 250 mm (168 in.). Travel of lifts conforming to 2.1.3 or shall not exceed 1 500 mm (60 in.). Travel of lifts conforming to 2.1.4 shall not exceed 600 mm (24 in.). Travel of lifts conforming to 2.1.6 shall not exceed 375 mm (15 in.), which poses a significant economic/financial hardship. Any interested person may file comments within 14 days of the publication of this notice with Division of Hotels and Restaurants, Bureau of Elevator Safety, 2601 Blair Stone Road, Tallahassee, Florida 32399-1013 (VW2026-160).

A copy of the Petition may be obtained by contacting: Division of Hotels and Restaurants, Bureau of Elevator Safety, 2601 Blair Stone Road, Tallahassee, Florida 32399-1013, elevators.dhr@myfloridalicense.com.

